**REQUEST FOR QUOTATION**

TO:

|  |  |  |  |
| --- | --- | --- | --- |
| All interested bidders |  | **Date of issue:** | September 14, 2020 |
|  | **File no.:** | AHEAD-0004 |
|  | **Contract title:** | Supply solar pump system and transmission line for well to elevated tank |
|  | **Closing date:** | September 27, 2020 at 3PM Kabul time |
|  | **For further information, please contact the Contracting Authority:** | Assistance for Health, Education and Development (AHEAD)  House # 12, Street # 9, Taimani, Kabul, Afghanistan  Contact person: Dr. Said Assadullah Fayaz  Tel: +937 700 502 211  Email:[procurement@ahead.org.af](mailto:procurement@ahead.org.af) |
|  |  | **Please note that the Quotations may be delivered to the Contracting Authority at the above address by in a sealed envelope clearly marked with the above File Number and the name of the submitting company.** | |

**AHEAD, Afghanistan invites you to submit a quotation for the following**

ANNEX 1

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Item | Description | Unit | Estimated Quantity | Required delivery date |
| 1 | Solar pump system and transmission line for well to Elevated Tank | LS | 2 | Oct 07, 2020 |

Solar pump system per wells.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SN | Item | Description | Quantity | Remark |
| 1 | Supply and installation of Submersible 7.5 Kw pump( Q – Discharge =3.611 lit/sec,Head =84m. Outside diameter of pum = To be able to instal in insid casing with the diameter of 6 inches easely, with high efficency inverter | 1.00 | No |  |
| 2 | Solar panels 280 watt sould mauch with IEC Standard. | 40.00 | NO |  |
| 3 | Solar panels stand steel,25 and 45 deg, Large (panels suport structure) Adjustable with doul access (harezantal and vertical) | 2.00 | set |  |
| 4 | Well probe sensor | 1.00 | set |  |
| 5 | wiring cost | 1.00 | set |  |
| 6 | Submercible drop cable (4\*1.5)mm2 from panels to solar pump کیبل برق از سولر پنیل الی پمپ | 100.00 | m |  |
| 7 | Cable (2\*1.5)mm2 کیبل برق | 100.00 | m |  |
| 8 | Conduct pipe | 100.00 | m |  |
| 9 | Wire tire white and black | 2.00 | PKT |  |
| 10 | Cable (1\*10)mm2 کیبل برق | 104.00 | m |  |
| 11 | Ground rod with copper Cable سیستم آرتنگ | 1.00 | set |  |
| 12 | Float switch | 1.00 | set |  |
| 13 | Supply and installation of solar pump set and solar panels انتقال ومونتاژ سبمرسیبل پمپ و سیستم سولر پنیل ها | 1.00 | set |  |
| 14 | Safty rope for holding of solar pump ریسمان پلاستیکی برای واتر پمپ | 170.00 | m |  |
| 15 | Supplying, installation, laying and fitting in place of High Density Polyethylene pipe (PE 100 PN 16 SDR 17), Outside Diameter: 63 mm, wall thickness 5.8 mm ,weight 1.06 kg/m, Best quality.پایپ پولی ایتیلین بقطر خارجی 63 ملی با فشارقابل برداشت 16 بار | 80.00 | m |  |
| 16 | Supply and installation of Polyethylene 90° bend, Size (63)mmزانوخم 90 درجه نوع پولی ایتیلین | 1.00 | No |  |
| 17 | Supply and installation of Galvanized Iron Paddle flange diameter 63 mm(clip on the top of the well to hold up the riser main pipe) کلیپب برای محکم نمودن پایپ و واتر پمپ چاه | 1.00 | No |  |
| 18 | Supply and installation of Gate valve (good quality) Nominal Diameter =2" best qualityگیت وال به قطردو انچ | 1.00 | No |  |
| 19 | Supply and installation of (good quility non return valve Dia =2" for riser main pipe in pump house, best quality with all related fittings تمبه والو به قطردو انچ | 1.00 | No |  |
| 20 | Supply and installaiton of Galvanized Iron (GI) pipe, inside diameter 2"پايپ آهني ملمع جست بقطر داخلي | 16.00 | m |  |
| 21 | Supply and installaiton of Mail threaded Adopter (MTA), Size (63x2") ادپتربقطر | 4.00 | No |  |
| 22 | Supply and installation of Galvanized Iron Socket, diameter 2"سامي آهني ملمع جست بقطر | 6.00 | No |  |
| 23 | Supply and installation of Galvanized Iron Nipple, diameter 2"اشتت آهني ملمع جست بقطر | 6.00 | No |  |
| 24 | Supply and installation of Galvanized Iron Elbow, diameter 2"زانو خم آهني ملمع جست بقطر | 3.00 | No |  |
| 25 | Supply and installation of Galvanized Iron Union 2"پیوند آهني ملمع جستی بقطر | 2.00 | No |  |

## Instructions

1. **Acknowledgement**

Upon receipt of the Request for Quotation please inform the Contracting Authority if you intend to submit a quotation. Please respond even if negative.

1. **General**

The goods to be purchased are for use by the Contracting Authority in its WASH Programme in Afghanistan, an intervention supported by NCA. The supplier can submit a quotation for one, several or all lots.

1. **Cost of quotation**

The supplier shall bear all costs associated with the preparation and submission of his quotation and the Contracting Authority will in no case be responsible or liable for these costs, regardless of the conduct or outcome of the negotiated procedure.

1. **Eligibility and qualification requirements**

Suppliers are not eligible if they are in one of the situations listed in article 15 of the General Terms and Conditions for Supply Contracts.

In the Quotation Submission Form suppliers shall attest that they meet the above eligibility criteria. If required by the Contracting Authority, the supplier whose quotation is accepted shall further provide evidence satisfactory to the Contracting Authority of its eligibility through certificates issued by competent authorities in its country of establishment or operation or, if such certificates are not available, through a sworn statement.

Suppliers shall also be requested to certify that they comply with article 13. “Child Labour and Forced Labour” and article 14 “Mines” of the General Terms and Conditions for Supply Contracts and with the Code of Conduct for Contractors.

To give evidence of their capability and adequate resources Suppliers shall provide the information and the documents requested by the Contracting Authority.

1. **Exclusion from award of contracts**

Contracts may not be awarded to Candidates who, during this procedure:

1. are subject to conflict of interest:
2. are guilty of misrepresentation in supplying the information required by the Contracting Authority as a condition of participation in the Contract procedure or fail to supply this information.
3. **Documents comprising the Request for Quotation**

The Supplier shall complete and submit the following document with his quotation:

1. The attached Quotation Submission Form
2. Valid Business License
3. Warranty letter for the solar panel and Guarantee for the electric pump
4. **Price**

The price quoted by the supplier shall not be subject to adjustments on any account except as otherwise provided in the conditions of the Contract.

Price shall be quoted in USD $.

**Tax**

**Withholding Tax on Subcontractor:**

Government withholding Tax: Pursuant to Article 72 in the Afghanistan Tax law effective March 21, 2009, NCA is required withhold “contractor” taxes from the gross amount payable to all Afghan for-profit subcontractor/vendors with aggregate amount of AFN 500,000.00 or greater and transfer this to the Ministry of Finance. In accordance with this requirement, NCA shall withhold 2% tax from all gross invoices from subcontractors/vendors under this Agreement with active AISA or Ministry of Commerce License. For subcontractors /vendors without active AISA or Ministry of Commerce license, NCA shall withhold seven percent 7% “contractor” tax per current Afghanistan Tax law.

1. **Validity**

Quotations shall remain valid and open for acceptance for 30 days after the closing date.

1. **Closing date**

Quotation must be received by the Contracting Authority as specified on page 1 not later than the closing date and time. Any quotations received after that will not be considered.

1. **Award of Contract and Criteria**

The Contracting Authority will award the Contract to the supplier whose quotation has been determined to be substantially responsive to this Request for Quotation (RFQ) and who has offered the lowest evaluated price, provided further that the supplier has the capability and resources to carry out the Contract effectively.

The Contracting Authority reserves the right to accept all or part of your quotation, whichever is in its best financial interest.

1. **Signature and entry in to force of the Contract**

Prior to the expiration of the period of the quotation validity, the Contracting Authority will notify the successful supplier in writing. Within five days of receipt of the Contract, not yet signed by the Contracting Authority, the successful supplier must sign and date the Contract and return it to the Contracting Authority. On signing the Contract, the successful supplier will become the Contractor and the Contract will enter into force once signed by the Contracting Authority.

If the successful supplier fails to sign and return the Contract and within the days stipulated, the Contracting Authority may consider the acceptance of the quotation to be cancelled without prejudice to the Contracting Authority's right to claim compensation or pursue any other remedy in respect of such failure, and the successful supplier will have no claim whatsoever on the Contracting Authority.

1. **Cancellation for convenience**

The Contracting Authority may for its own convenience and without charge or liability cancel the RFQ at any stage.

### Special conditions

1. **Scope of Supply Solar System**

The subject of the contract is the supply, supply and installation of the supplies described in the Price and Technical Data Form in Annex 1.

1. **After sales Service**

The supplier shall warrant that the solar system will work normally and sufficiently and if repair is need for any part of the salary system should promptly without any delay repair it. This warranty/ guaranty should be for the warranty period of ( ) after the installation of the solar system (Pump and Solar panels) in Kabuli Payen and Qarcha Blaq located in Hazrat Sultan district of Samangan province.

1. **Installation and Commissioning**

The supplier shall include in his quotation a complete and detailed plan for start-up and commissioning of the

Solar System at the project site and shall clearly state what is included in the price and what costs are not

included. Any costs that can be reasonably foreseen as necessary for the installation and commissioning of the Solar System that are not specifically included or excluded in the price, will be deemed to be included in the overall price

1. **Payment**

Payment will be made upon receipt of the following documents and within 30 days after receipt of goods:

**QUOTATION SUBMISSION FORM**

**Price schedule**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | Description | **Unit** | **Qty** | **Currency USD $** | |
| **Unit Price** | **Total Price** |
| 1 | Solar pump system and transmission line for well to Elevated Tank | System | 2 |  |  |

Solar pump system per wells.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | **Description** | **Unit** | **Qty** | **Currency USD $** | |
| **Unit Price** | **Total Price** |
| 1 | Supply and installation of Submersible 7.5 Kw pump( Q – Discharge =3.611 lit/sec,Head =84m. Outside diameter of pum = To be able to instal in insid casing with the diameter of 6 inches easely, with high efficency inverter | No | 1.00 |  |  |
| 2 | Solar panels 280 watt sould mauch with IEC Standard. | NO | 40.00 |  |  |
| 3 | Solar panels stand steel,25 and 45 deg, Large (panels suport structure) Adjustable with doul access (harezantal and vertical) | set | 2.00 |  |  |
| 4 | Well probe sensor | set | 1.00 |  |  |
| 5 | wiring cost | set | 1.00 |  |  |
| 6 | Submercible drop cable (4\*1.5)mm2 from panels to solar pump کیبل برق از سولر پنیل الی پمپ | m | 100.00 |  |  |
| 7 | Cable (2\*1.5)mm2 کیبل برق | m | 100.00 |  |  |
| 8 | Conduct pipe | m | 100.00 |  |  |
| 9 | Wire tire white and black | PKT | 2.00 |  |  |
| 10 | Cable (1\*10)mm2 کیبل برق | m | 104.00 |  |  |
| 11 | Ground rod with copper Cable سیستم آرتنگ | set | 1.00 |  |  |
| 12 | Float switch | set | 1.00 |  |  |
| 13 | Supply and installation of solar pump set and solar panels انتقال ومونتاژ سبمرسیبل پمپ و سیستم سولر پنیل ها | set | 1.00 |  |  |
| 14 | Safty rope for holding of solar pump ریسمان پلاستیکی برای واتر پمپ | m | 170.00 |  |  |
| 15 | Supplying, installation, laying and fitting in place of High Density Polyethylene pipe (PE 100 PN 16 SDR 17), Outside Diameter: 63 mm, wall thickness 5.8 mm ,weight 1.06 kg/m, Best quality.پایپ پولی ایتیلین بقطر خارجی 63 ملی با فشارقابل برداشت 16 بار | m | 80.00 |  |  |
| 16 | Supply and installation of Polyethylene 90° bend, Size (63)mmزانوخم 90 درجه نوع پولی ایتیلین | No | 1.00 |  |  |
| 17 | Supply and installation of Galvanized Iron Paddle flange diameter 63 mm(clip on the top of the well to hold up the riser main pipe) کلیپب برای محکم نمودن پایپ و واتر پمپ چاه | No | 1.00 |  |  |
| 18 | Supply and installation of Gate valve (good quality) Nominal Diameter =2" best qualityگیت وال به قطردو انچ | No | 1.00 |  |  |
| 19 | Supply and installation of (good quility non return valve Dia =2" for riser main pipe in pump house, best quality with all related fittings تمبه والو به قطردو انچ | No | 1.00 |  |  |
| 20 | Supply and installaiton of Galvanized Iron (GI) pipe, inside diameter 2"پايپ آهني ملمع جست بقطر داخلي | m | 16.00 |  |  |
| 21 | Supply and installaiton of Mail threaded Adopter (MTA), Size (63x2") ادپتربقطر | No | 4.00 |  |  |
| 22 | Supply and installation of Galvanized Iron Socket, diameter 2"سامي آهني ملمع جست بقطر | No | 6.00 |  |  |
| 23 | Supply and installation of Galvanized Iron Nipple, diameter 2"اشتت آهني ملمع جست بقطر | No | 6.00 |  |  |
| 24 | Supply and installation of Galvanized Iron Elbow, diameter 2"زانو خم آهني ملمع جست بقطر | No | 3.00 |  |  |
| 25 | Supply and installation of Galvanized Iron Union 2"پیوند آهني ملمع جستی بقطر | No | 2.00 |  |  |
|  | Sub Total Incl. Tax: | | | |  |
|  | Freight to Hazrat Sultan district of Samangan province (Qarcha Blaq and Kabuly Bayen) | | | |  |
|  | Grand Total Incl. Tax: | | | |  |

Any subsequent procurement related to this Quotation will be subject to the Contracting Authorities General Terms and Conditions for Supply Contracts and the Code of Conduct for Contractors available through the below link. Printed versions are available on request.

<https://www.kirkensnodhjelp.no/en/about-nca/for-contractors/>

After having read this Request for Quotation <reference> on behalf of my company/business, I hereby:

* Accept, without restrictions, all the provisions in the Request for Quotation including General Terms and Conditions for Supply Contracts with annexes.
* Provided that a contract is issued by the Contracting Authority we hereby commit to furnish any or all items at the price offered and deliver same to the designated points within the delivery time stated above.
* Certify and attest that we meet the eligibility criteria stated in the Instructions.
* Certify and attest compliance with the Code of Conduct for Contractors.

This declaration will be confirmed in the Contract and misrepresentation will be regarded as grounds for termination.

Signature and stamp:

Signed by:

|  |  |
| --- | --- |
| **The Contractor** |  |
| Name of the company |  |
| Address |  |
| Telephone no. |  |
| E-mail: |  |
| Name of contact person |  |
| Date: |  |