## 

Rural Rehabilitation

Association for Afghanistan

(RRAA)

**REQUEST FOR QUOTATION**

TO:

|  |  |  |  |
| --- | --- | --- | --- |
| **All interested Company** |  | **Date of issue:** | Oct ,10,2019 |
|  | **File no:** | 04-110152-3 |
|  | **Contract title:** | Provision of Pipe, fitting,and Transporting to the site |
|  | **Closing date:** | 23/Oct/2019 |
|  | **For further information, please contact the Contracting Authority:** | Darulaman Road Opposite of Ministry of commerce, Ayub khan mina District No 7 House #669  Contact person: Hamed  Tel: 0093(0)772630093/0700051138  Fax: N/A  Email: [hoprocurement@rraa,org.af](mailto:hoprocurement@rraa,org.af)  For Technical information  Eng. Wali khan  Tel: 0093(0)774950200  Email:  [engwalikhan13@yahoo.com](mailto:waisguzar@hotmail.com) |
|  |  | **Please note that the Quotations may be delivered to the Contracting Authority at the above address by in a sealed envelope clearly marked with the above File Number and the name of the submitting company. On Date: Oct,23,2019**  **Time; from1:00 PM- 2:00 PM** | |

**Rural ReHEBILATATION ASSOCIATION OF aFGHANISTAN (rraa)invites you to submit a quotation for the following goods with delivery to THE project site (Trinkot district of Urozgan province)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | **Description** | Origin of goods | Required delivery date | **Unit** | **Quantity** |
| 1 | Solar panel : Poly /Mono 280 Watt With german IEC Standard .  With 10 years performance Waranty and 25 Years Power Waranty According Data Sheet of Solar Penals. |  |  | Panel | 60 |
| 2 | Solar Pump :   * Power 2.1 KW * Flow Rate .   1-60 Meters head:8000 Liters/hour.  2-80 Meters head :7000 Litters /hour.  3-100 Meters head :5000 Litters /hour.  With two years Guarantee. |  |  | Pcs | 6 |
| 3 | Wire :Copper , 2x4mm |  |  | Meter | 600 |
| 4 | Pipe: PE, high class, PE 100 PN 10, 1.5 Inch |  |  | M | 540 |
| 5 | Switch box for solar and Pump |  |  | Pcs | 6 |
| 6 | Rope :Plastic 10 mm |  |  | M | 480 |
| 7 | Transportation to project site. |  |  | Ls | 6 |
| 8 | installation of solar systems in site. |  |  | Ls | 6 |
| 9 | Adjustable Solar Mounting Frame for 10 Pcs solar Panels |  |  | Frame | 6 |

## Instructions

1. **Acknowledgement**

Upon receipt of the Request for Quotation please inform the Contracting Authority if you intend to submit a quotation. Please respond even if negative.

1. **General**

The goods to be purchased are for use by the Contracting Authority in its Water Supply Programme in Trinkot District of Urozgan Province Afghanistan, an intervention supported by NCA. The supplier can submit a quotation for one, several or all lots.

1. **Cost of quotation**

The supplier shall bear all costs associated with the preparation and submission of his quotation and the Contracting Authority will in no case be responsible or liable for these costs, regardless of the conduct or outcome of the negotiated procedure.

1. **Eligibility and qualification requirements**

Suppliers are not eligible if they are in one of the situations listed in article 15 of the General Terms and Conditions for Supply Contracts.

In the Quotation Submission Form suppliers shall attest that they meet the above eligibility criteria. If required by the Contracting Authority, the supplier whose quotation is accepted shall further provide evidence satisfactory to the Contracting Authority of its eligibility through certificates issued by competent authorities in its country of establishment or operation or, if such certificates are not available, through a sworn statement.

Suppliers shall also be requested to certify that they comply with article 13. “Child Labour and Forced Labour” and article 14 “Mines” of the General Terms and Conditions for Supply Contracts and with the Code of Conduct for Contractors.

To give evidence of their capability and adequate resources Suppliers shall provide the information and the documents requested by the Contracting Authority.

1. **Exclusion from award of contracts**

Contracts may not be awarded to Candidates who, during this procedure:

1. are subject to conflict of interest:
2. are guilty of misrepresentation in supplying the information required by the Contracting Authority as a condition of participation in the Contract procedure or fail to supply this information.
3. **Documents comprising the Request for Quotation**

The Supplier shall complete and submit the following document with his quotation:

1. The attached Quotation Submission Form
2. Suppliers technical specifications.
3. Copies of any registration certificates as required by national legislation or competent authorities including company registration certificates and membership certificates of any relevant professional bodies (Shall only be submitted if you have not delivered to the Contracting Authority before)
4. References that we may contact for further background information of your company. (Shall only be submitted if you have not delivered to the Contracting Authority before)
5. **Price**

The price quoted by the supplier shall not be subject to adjustments on any account except as otherwise provided in the conditions of the Contract.

Price shall be quoted in USD.

***Tax***

Withholding Tax on Subcontractor:

Government withholding Tax: Pursuant to Article 72 in the Afghanistan Tax law effective March 21, 2009, NCA is required withhold “contractor” taxes from the gross amount payable to all Afghan for-profit subcontractor/vendors with aggregate amount of AFN 500,000.00 or greater and transfer this to the Ministry of Finance. In accordance with this requirement, NCA shall withhold 2% tax from all gross invoices from subcontractors/vendors under this Agreement with active AISA or Ministry of Commerce License. For subcontractors /vendors without active AISA or Ministry of Commerce license, NCA shall withhold seven percent 7% “contractor” tax per current Afghanistan Tax law.

1. **Validity**

Quotations shall remain valid and open for acceptance for 5days still the closing date.23/Oct/2019

1. **Closing date**

Quotation must be received by the Contracting Authority as specified on page 1 not later than the closing date and time. Any quotations received after that will not be considered.

1. **Award of Contract and Criteria**

The Contracting Authority will award the Contract to the supplier whose quotation has been determined to be substantially responsive to this Request for Quotation (RFQ) and who has offered the lowest evaluated price, provided further that the supplier has the capability and resources to carry out the Contract effectively.

The Contracting Authority reserves the right to accept all or part of your quotation, whichever is in its best financial interest.

1. **Signature and entry in to force of the Contract**

Prior to the expiration of the period of the quotation validity, the Contracting Authority will notify the successful supplier in writing.

Within 2 days of receipt of the Contract, not yet signed by the Contracting Authority, the successful supplier must sign and date the Contract and return it, to the Contracting Authority. On signing the Contract, the successful supplier will become the Contractor and the Contract will enter into force once signed by the Contracting Authority.

If the successful supplier fails to sign and return the Contract and within the days stipulated, the Contracting Authority may consider the acceptance of the quotation to be cancelled without prejudice to the Contracting Authority's right to claim compensation or pursue any other remedy in respect of such failure, and the successful supplier will have no claim whatsoever on the Contracting Authority.

1. **Cancellation for convenience**

The Contracting Authority may for its own convenience and without charge or liability cancel the RFQ at any stage.

### Special conditions

1. **Scope of Supply**

The subject of the contract is the supply and delivery of all mentioned goods to project site (Trinket district of Urozgan Province) supplies described in the Price and Technical Data Form in Annex 1.

1. **A. (After sales Service)**

The supplier shall ensure availability of purchased material after sales service; supplier must have a.

- Solar panel: Poly /Mono 280 Watt with German IEC Standard.

With 10 years Performance Warranty and 25 Years Power Warranty According Data Sheet of Solar Penal.

- Solar Pump:

• Power 2.1 KW

• Flow Rate.

1-60 Meters head:8000 Litters/hour.

2-80 Meters head :7000 Litters /hour.

3-100 Meters head :5000 Litters /hour.

With two years Guarantee.

1. **Minimum Eligibility Criteria**

The supplier must complete the following documents to be eligible for this procurement process:

* Accept NCA General Terms and Conditions and Code of Conduct
* Attached a Valid Business License /AISA certificate
* Complete the RFQ sign and stamp.
* At least 3 reference to be provided.
* Performance Warranty or Guarantee letter for Solar panel /other equipment’s separately in company letter head sign and stamped.

1. **Payment**

Payment will be made upon receipt of the following documents and within 10 days after receipt of goods:

1. Invoice (one original)
2. Proof of delivery Waybill.

**QUOTATION SUBMISSION FORM**

**Price schedule**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Item** | **Description** | **Unit** | **Qty** | **Currency** | |
| **Unit Price (USD)** | **Total Price(USD)** |
| 1 | Solar panel : Poly /Mono 280 Watt With german IEC Standard .  With 10 years performance Waranty and 25 Years Power Waranty According Data Sheet of Solar Penals | Panel | 60 |  |  |
| 2 | Solar Pump :  •Power 2.1 KW  •Flow Rate .  1-60 Meters head:8000 Liters/hour.  2-80 Meters head :7000 Litters /hour.  3-100 Meters head :5000 Litters /hour.  With two years Guarantee. | Pcs | 6 |  |  |
| 3 | Wire :Copper , 2x4mm | M | 600 |  |  |
| 4 | Pipe: PE, high class, PE 100 PN 10, 1.5 Inch | M | 540 |  |  |
| 5 | Switch box for solar and Pump | Pcs | 6 |  |  |
| 6 | Rope :Plastic 10 mm | M | 480 |  |  |
| 7 | Transportation to project site. | LS | 6 |  |  |
| 8 | installation of solar systems in site. | LS | 6 |  |  |
| 9 | Adjustable Solar Mounting Frame for 10 Pcs solar Panels | Frame | 6 |  |  |
| **Total price with tax** | | | | |  |
| **Tax( %)** | | | | |  |
| **Total Price Without Tax (USD)** | | | | |  |

***Note:*** *The cost should include all the taxes and transportation to the site*

|  |  |
| --- | --- |
|  | **Information to be entered by supplier in the below columns** |
| Please state name of Manufacturer |  |
|  |  |
| **After sales service and warranty service** |  |
| Please state full contact details of the local after sales service. |  |
|  |  |
| **Delivery date** |  |
| Delivery time to final destination | days |
| **Technical specification** |  |
| Complete technical description is attached (Y/N) |  |
|  |  |
| **References** |  |
| A reference list is attached (shall only be submitted if supplier has not delivered to the Contracting Authority before) |  |
|  |  |
| **CSR information** |  |
| Does your company have CSR related policies in place – e.g. health and safety policy, HR policy, staff policy, energy policy, climate policy or is a member of Global Compact. Please state which policies. |  |
| Is your company e.g. **ISO** 26000/50001/14000 certified or SA8000 certified? Please state which. |  |
| Does your company have a Code of Conduct? |  |

Suppliers are requested to complete the following form

The following technical specifications are provided in the format of a checklist. They are compulsory as minimum standard and will be the only basis for the Contracting Authority to assess the technical compliance of the equipment presented in the quotations. Deviations from the specifications may be considered only if deemed to be in the best interest of the Contracting Authority.

**technical data form**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Item no.:** | **Parameter** | **Characteristics (Contracting Authorities minimum requirement)** | **Comply (Y / N)** | **Deviations, if any, to be described in this column** |
| **1** | **Description** | Supply, installation and transportation of Solar systems in project site. |  |  |
|  |  |  |  |
| **Specifications** | Refer to Quotation submission form |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
| **(Option: Certificates)** | (Option: Please specify and enclose any quality accreditation - ISO 9000 2000 or equivalent held by the manufacturer of the offered products) |  |  |
| **3** | **Guaranty** | Mentioned the duration |  |  |
| **4** | **Warranty** | Mentioned the duration |  |  |

Manufacturers’ names, catalogue numbers and model designations appearing in the list are for reference only. Quotations for other equipment that is equal in function, quality and performance to that listed will be given full consideration.

Any subsequent procurement related to this Quotation will be subject to the Contracting Authorities General Terms and Conditions for Supply Contracts and the Code of Conduct for Contractors available through the below link. Printed versions are available on request.

<https://www.kirkensnodhjelp.no/en/about-nca/for-contractors/>

Do you accept NCA General Terms and Conditions and Code of Conduct? Yes 󠅾󠅾 No 󠅾󠅾

After having read this Request for Quotation following goods on behalf of my company/business, I hereby:

* Accept, without restrictions, all the provisions in the Request for Quotation including General Terms and Conditions for Supply Contracts with annexes.
* Provided that a contract is issued by the Contracting Authority we hereby commit to furnish any or all items at the price offered and deliver same to the designated points within the delivery time stated above.
* Certify and attest that we meet the eligibility criteria stated in the Instructions.
* Certify and attest compliance with the Code of Conduct for Contractors.

This declaration will be confirmed in the Contract and misrepresentation will be regarded as grounds for termination.

Signature and stamp:

Signed by:

|  |  |
| --- | --- |
| **The Contractor** |  |
| Name of the company |  |
| Address |  |
| Telephone no. |  |
| E-mail: |  |
| Name of contact person |  |
| Date: |  |